**program 25 :Write an assembly language program to swap two 8-bit datausing 8085 processor.**

**PROGRAM :**

LDA 0000

MOV B,A

LDA 0001

MOV C,A

STA 0003

MOV A,B

STA 0004

HLT

